* + - 1. SNAP SWITCHES
				1. Comply with NEMA WD 1, UL 20 and Federal Specification W-S-896. Constructed from chemical and impact-resistant thermoplastics, nickel-plated mounting strap, and solid brass contacts. Single-piece toggle is made of chemical-resistant thermoplastics. Catalog numbers in subparagraphs below are for 20-A devices; revise catalog numbers if 15-A devices are desired.
				2. Switches, 120/277 V, 20 A. Prewired pigtail connectors that accommodate Fed Spec switches are approved. Must be crimped and welded terminal right angle application connector.

See Editing Instruction No. 1 in the Evaluations for cautions about naming manufacturers and products. Retain one of two subparagraphs and list of manufacturers below. See Division 01 Section "Product Requirements."

Available Products: Subject to compliance with requirements, products that may be incorporated into the Work include, but are not limited to, the following:

Products: Subject to compliance with requirements, provide one of the following:

Pass & Seymour; PS20AC1 (single pole), PT20AC1 (single pole – use with PTS6STR3 prewired pigtail connector), PS20AC2 (two pole), PS20AC3 (three way), PT20AC3 (three way – use with PTS6STR4 prewired pigtail connector), PS20AC4 (four way).

<**Insert manufacturer's name; catalog numbers.**>