* + - 1. SNAP SWITCHES
         1. Comply with NEMA WD 1, UL 20 and Federal Specification W-S-896. Constructed from chemical and impact-resistant thermoplastics, nickel-plated mounting strap, and solid brass contacts. Single-piece toggle is made of chemical-resistant thermoplastics. Catalog numbers in subparagraphs below are for 20-A devices; revise catalog numbers if 15-A devices are desired.
         2. Illuminated, 20 A:

See Editing Instruction No. 1 in the Evaluations for cautions about naming manufacturers and products. Retain one of first two subparagraphs and list of manufacturers below. See Division 01 Section "Product Requirements."

Available Products: Subject to compliance with requirements, products that may be incorporated into the Work include, but are not limited to, the following:

Products: Subject to compliance with requirements, provide one of the following:

Pass & Seymour; PS20AC1IL.

<**Insert manufacturer's name; catalog numbers.**>

Description: Single pole, with neon-lighted handle, illuminated when switch is "ON."