##

The component automatically configures itself to collect data from every available recorder in every device or software component and inputs this data into the database. is typically run only on the Primary workstation.

Most systems use only a single which is automatically configured to perform all required logging functions. The default configuration works for most systems. Situations where changes may be required include systems with large numbers of devices with logs, systems with primary and secondary servers or cases where only specific devices and/or logs need to be monitored for new records. If any of these situations apply to your system, contact for more information on the operation of , its different modes of operation, and the functions of its internal components.