## commands

The following summarizes the commands available in the :

File > Save: Saves your changes. A copy of the changes are saved for future reference, in a comma-separated value (.csv) data file in the ...\config\Diagnostic\\ folder.

File > Exit: Closes the .

Edit > Reset: Clears the modifications made since the last save.

Edit > Delete: Deletes the selected rows.

Edit > Rename Source: Lets you change the name of an Assigned Source. See "Renaming the Assigned Source" on page 1.

Edit > Update Historical Data: Opens the “Update Historical Data” window that allows you to open a previously-saved source-measurement definition data file (with a .csv file extension), for the purpose of updating existing data in the database. You can also manually add, edit or delete data entries. See "Updating the Historical Data at a Later Time" on page 1.

View > Refresh: Loads the current downstream definitions from the database. Functionally the same as Edit > Reset, as this command clears the modifications made since the last save.

View > Options: Displays the Options dialog where you can change the settings that control what level of detail is displayed for the source-measurement definitions.

View > Select Physical Sources: Displays the Select Physical Sources dialog where you can select which physical devices you want displayed in the .