## Time synchronization blackout

Time synchronization blackout is defined as a period when time synchronization cannot occur. Utilities often record power usage at regular, predetermined intervals. For example, the utility may schedule a recording every five minutes during an hour period (that is, 5, 10, 15, 20,..., 55, 60). If a time sync moves the meter clock forward, the meter may miss one of the recording intervals. If a time sync moves the meter clock backwards, the meter may get two records with the same timestamp. The time synchronization blackout feature seeks to protect the time before and after these recording intervals by not sending out any time sync signals at those times.

has time synchronization blackouts enabled automatically even though time syncing is disabled by default in . The blackout intervals are every five minutes as follows: 0, 5, 10, 15, 20, 25, 30, 35, 40, 45, 50, 55. Each blackout is 2 minutes and 30 seconds in duration. This duration is distributed evenly before and after the interval. The diagram below illustrates the time synchronization blackout feature in .

If a regularly scheduled time sync is not sent because of a blackout interval, the software continues trying to send the time synchronization signal every 15 seconds until the blackout period expires and the time sync is sent.

### Changing default blackout settings

To change the default settings for the interval or the blackout duration, you must edit the registry of the computer where is installed. Changing the default registry settings should be performed only by personnel with a thorough knowledge of their computer's operating system and registry entries.

notice

irreversible operating system damage or data corruption

Registry edits must be performed only by qualified and experienced personnel.

Before making any changes, back up your system registry in a network folder or other remote location.

Failure to follow these instructions can result in irreparable damage to your computer's operating system and all existing data.

There are two registry entries that control the time-synchronization blackout behavior.

For 32-bit servers, create the following registry `REG_DWORD` values under the HKEY_LOCAL_MACHINE\Software\\\version_number key.

For 64-bit servers, create the following registry `REG_DWORD` values under the HKEY_LOCAL_MACHINE\Software\Wow6432Node\\\version_number key.

##### TimesyncBlackoutInterval_mins

> Default value: 5

> This entry is specified in minutes. It must have a value greater than 1 in order for time-synchronization blackouts to occur. A value of 60 or greater configures blackouts to occur once an hour.

##### TimesyncBlackoutDuration_secs

> Default value: 150 (2 minutes 30 seconds in seconds)

> This entry is specified in seconds. A value of 0 (zero) disables the blackout feature. This entry cannot have a value greater than or equal to 3600 (one hour).

Note

If you want to disable the blackout feature but keep time synchronization enabled, set the TimesyncBlackoutDuration_secs register to 0.

Do not use the following settings. They disable both the blackout feature as well as time synchronization in general.

TimesyncBlackoutInterval_mins < 1

TimesyncBlackoutDuration_secs >= 3600 (1 hour)

TimesyncBlackoutDuration_secs (the value converted to minutes) >=
TimesyncBlackoutInterval_mins

To disable time synchronization for a particular device, use Management Console. Refer to "Enabling or customizing time synchronization" on page 1.

#### Time-synchronization blackout considerations

Remember to specify TimesyncBlackoutInterval_mins in minutes and TimesyncBlackoutDuration_secs in seconds.

If your blackout values conflict or are out of range, an error is sent to the system log database. If time synchronization signals are not occurring, check the system log to see if there’s an error message about your blackout values.