,Model##other##text,Depth##length##inches,Height##length##inches,Width##length##inches,Description##other##text,Product Page URL##other##text,Product Material##other##text,z Bottom Side Holes##other##,z Bottom Squres##other##,z Center Circle##other##,z Center Circle Radius##length##inches,z Center Offset##length##inches,z Center Offset Holes##other##,z Center Square (68)##other##,z Center Square Length (68)##length##inches,z Center Square Width (68)##length##inches,z Inner Plate Length##length##inches,z Inner Plate Top Offset##length##inches,z Inner Sockets##other##,z Inner Tile##other##,z Inner Tile Width##length##inches,z Inside Marks Length##length##inches,z Is Center Plate##other##,z Is Side Plate##other##,z Mark Width##length##inches,z Middle Holes##other##,z Middle Mark Offset##length##inches,z Middle Marks Length##length##inches,z Middle Squares (68)##other##,z Multiple Squares##other##,z Not Seperate Squares##other##,z Not Square Rows##other##,z Outlet (68)##other##,z Outside Marks Length##length##inches,z Seperate Squares##other##,z Set 1##other##,z Set 2##other##,z Small Center Square (68)##other##,z Square Rows##other##,z Top Side Holes##other##,z Top Square##other##
Center Mount-8 Port Comm,6ACT8A,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Eight Ports of Communication Devices",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6act8a-device-plate.aspx#.UDLAuqOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,0,1.4,2,4.375,0.25,0,1,1.495964803,0.944,1,0,0.748,0,0,2.832,0,1,1,1,0,2.832,0,1,0,0,0,0,0
Center Mount-AAP,6AAP,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Two Extron® Electronics AAP Style
 Plates",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6aap-device-plate.aspx#.UDLBlKOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,1,0,1.0625,2,2.75,1.063,0,1,1.375,0,1,0,0.75,0,0,0,0,0,1,1,0,0,0,1,0,0,0,0,0
Center Mount-Blank,6B,0.125,4.875,2.188,"6AT Center Mount Device Plate, Blank",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6b-device-plate.aspx#.UDLBlqOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,0,1.4,2,4.375,0.25,0,0,1.495964803,0.625,1,0,1.09375,0,0.3125,1.875,0,0,0,0,0,3.125,0,0,0,0,0,0,0
Center Mount-Combination,6MAAP2A,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Three Extron®
 Electronics MAAP Style Plates and Two Ports of Communication Devices",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6maap2a-device-plate.aspx#.UDLAsqOX_RY,Paint - Wiremold - White,0,1,0,0.6875,0.812,0,0,1.4,2,4.313,0.25,0,0,1.438,0.625,1,0,1.09375,0,0.3125,1.875,0,0,0,0,0,3.125,0,0,1,0,0,1,1
Center Mount-Decorator,6DEC,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Decorator Style Devices",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6dec-device-plate.aspx#.UDLAqqOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,0,1.4,2,2.626,1.125,0,1,1.303,0,1,0,0,0,0,0,0,0,1,1,0,0,0,1,0,0,0,0,0
Center Mount-Duplex,6DP,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Standard 20A Duplex Receptacle or Duplex Turnlok Receptacle",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6dp-device-plate.aspx#.UDLCgKOX_RY,Paint - Wiremold - White,0,0,1,0.063,0.812,0,0,1.4,2,4.375,0.25,1,0,1.495964803,0,1,0,0,1,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
Center Mount-MAAP,6MAAP,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Six Extron® Electronics MAAP Style Plates",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6maap-device-plate.aspx#.UDLBfqOX_RY,Paint - Wiremold - White,1,0,0,0.6875,0.812,0,0,1.4,2,4.375,0.25,0,1,1.495964803,0.688,1,0,0,0,0,2.064,0,0,1,1,0,3.44,0,1,0,0,0,1,0
Center Mount-Mosaic,6MOS,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Two Standard [45mm X 45mm] or One Standard [45mm X 90mm] Mosaic Style Devices",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6mos-device-plate.aspx#.UDLCgqOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,0,1.4,2,3.375,0.75,0,1,1.495964803,1.688,1,0,0,0,0,0,0,0,1,1,0,0,0,1,0,0,0,0,0
Center Mount-Mosaic British Standard,6MOSBS,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Two Mosaic British Standard Devices",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6mosbs-device-plate.aspx#.UDLAsKOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,0,1.4,2,4.39,0.2421875,0,1,1.495964803,2.32,1,0,0,0,0,2.32,0,0,0,1,0,2.32,1,1,0,0,0,0,1
Center Mount-ORT Series II,6SER,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Four Ortronics® Series II Dual Modular Inserts",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6ser-device-plate.aspx#.UDLBgaOX_RY,Paint - Wiremold - White,0,0,0,0.6875,1.062,0,0,1.4,2,3.875,0.25,0,1,1.495964803,0.775,1,0,0,0,0,0.775,0,0,1,1,0,2.325,0,1,0,0,0,0,0
Center Mount-ORT TracJack,6TRAC,0.125,4.875,2.188,"6AT Center Mount Device Plate, Accepts Eight Ortronics® TracJack Devices",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6trac-device-plate.aspx#.UDLBQaOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,0,1.4,2,3.7,0.588,0,1,1.6,0.74,1,0,0.87,0,0,2.22,0,0,1,0,0,2.22,0,1,0,0,1,0,0
Center Mount-Single Rec S1,6S1,0.125,4.875,2.188,"6AT Center Mount Device Plate, Receptacle Opening 1 3/8"" [35mm]",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6s1-device-plate.aspx#.UDLBfKOX_RY,Paint - Wiremold - White,0,0,1,0.6875,0.812,0,0,1.4,2,4.375,0.25,0,0,1.495964803,0,1,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
Center Mount-Single Rec S2,6S2,0.125,4.875,2.188,"6AT Center Mount Device Plate, Receptacle Opening 1 9/16"" [40mm]",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/6s2-device-plate.aspx#.UDLAv6OX_RY,Paint - Wiremold - White,0,0,1,0.7815,0.812,0,0,1.4,2,4.375,0.25,0,0,1.496,0,1,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
Side Mount-2 Port Comm,682A,0.125,1.625,3,"6AT Side Mount Device Plate, Accepts Two Ports of Communication Devices",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/682a-device-plate.aspx#.UDLAyaOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.647625,0,1,1.063,2,4.375,0.25,0,0,1.495964803,0,0,1,0.906,0,0,0,1,0,0,0,0,0,0,1,0,0,0,0,0
Side Mount-Blank,68B,0.125,1.625,3,"6AT Side Mount Device Plate, Blank",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/68b-device-plate.aspx#.UDLCdaOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,0,1.063,2,4.375,0.25,0,0,1.495964803,0.625,0,1,1.09375,0,0,1.875,0,0,0,0,0,3.125,0,0,0,0,0,0,0
Side Mount-Duplex,68REC,0.125,1.625,3,"6AT Side Mount Device Plate, Two Proprietary 20AMP Power Receptacles",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/68rec-20a-duplex-receptacles.aspx#.UDLBjKOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.674,0,0,1.063,2,4.375,0.25,0,0,1.495964803,0,0,1,1.188,0,0,0,0,0,0,0,1,0,0,1,0,0,0,0,0
Side Mount-Duplex 25,68REC-25,0.125,1.625,3,"6AT Side Mount Device Plate, Two Proprietary 20AMP Power Receptacles with 25' Leads",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/68rec-25-20a-duplex-receptacles.aspx#.UDLBbaOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.674,0,0,1.063,2,4.375,0.25,0,0,1.495964803,0,0,1,1.188,0,0,0,0,0,0,0,1,0,0,1,0,0,0,0,0
Side Mount-MAAP,68MAAP,0.125,1.625,3,"6AT Side Mount Device Plate, Accepts Two Extron® Electronics MAAP Device
 Plates",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/68maap-device-plate.aspx#.UDLBcaOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.812,0,1,1.4,1.45,4.375,0.25,0,0,1.495964803,0.7,0,1,0,0,0,0.7,0,0,0,0,0,0.7,0,1,0,1,0,0,0
Side Mount-Pass Through,682A-PT,0.125,1.625,3,"6AT Side Mount Device Plate, Allows Communication Cabling to Pass Through",http://www.legrand.us/wiremold/poke-thru-devices/recessed-poke-thru-devices/evolution-6at-poke-thru-device/682a-pt-device-plate.aspx#.UDLAOaOX_RY,Paint - Wiremold - White,0,0,0,0.6875,0.632,0,1,1.063,2,4.375,0.25,0,0,1.495964803,0,0,1,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0
